# ECE 385

Fall 2021

Experiment #6

# Lab 6

**Simple Computer SLC-3.2 in SystemVerilog**

Guanshujie Fu 3190110666

Xiaomin Qiu 3190110717

Lab Section D231 18:00 – 21:00

TA: Yuchuan Zhu

1. **Introduction**
   1. Summarize the basic functionality of the SLC-3 processor

The SLC-3 processor is a subset of the LC-3 ISA, a 16-bit processor with 16-bit Program Counter. The processor could load/store data, jump to specific instructions, play arithmetic and logic calculation, and can be paused. It takes instructions from RAM and executes them with data registers.

1. **Written Description and Diagrams of SLC-3**
   1. Summary of Operation
      1. Describe in words how the SLC-3 performs its functions. In particular, you should describe the Fetch-Decode-Execute cycle as well as the various instructions the processor can perform.

The SLC-3 has three stages, FETCH, DECODE and EXCUTE, it could perform ADD, ADDi, AND, ANDi, NOT, BR, JMP, JSR, LDR, STR, PAUSE commands based on the instructions stored in SRAM.

The first stage is FETCH. The SLC-3 will store the value in PC register to MAR, the memory address to read the instruction from. Then store M[MAR] into MDR, the instruction read form the memory, and then pull the MDR value into the IR register which provides instructions and datapath with other necessary data. To finish Fetch, the PC register will be incremented.

The second stage is DECODE The SLC-3 will read the instructions stored in IR and send them to the Instruction Sequencer/Decoder which will decode it to determine the type of the instruction and generate the control signals to execute in proper order. IR[15:12] specifies the opcodes and IR[11:0] will be used to determine the registers address or offset number.

The third stage is EXCUTE. The SLC-3 will perform the operation based on the signals from the Instruction Sequencer/Decoder and write the result to the destination or memory. Operations include sending signal to ALU to perform logic calculations or loading/storing to the SRAM or JUMP/Branch to the specific locations.

Then the SLC-3 will fetch again.

* 1. Written Description of all .sv Modules

|  |  |
| --- | --- |
| **Modules** | **Synchronizers.sv** |
| Inputs | logic [15:0] S,  logic Clk, Reset, Run, Continue,  (inout wire [15:0] Data) |
| Outputs | logic [11:0] LED,  logic [6:0] HEX0, HEX1, HEX2, HEX3, HEX4, HEX5, HEX6, HEX7,  logic CE, UB, LB, OE, WE,  logic [19:0] ADDR, |
| Description | These are built by D flip-flops. Data is stored until it is on the positive edge of clock and then data will go from D to Q. |
| Purpose | These are synchronizers required for bringing asynchronous signals into the FPGA and make them executing signal synchronously. |

|  |  |
| --- | --- |
| **Modules** | **SEXT.sv** |
| Inputs | input logic [15:0] IR |
| Outputs | output logic [15:0] SEXT0\_10,  output logic [15:0] SEXT0\_8,  output logic [15:0] SEXT0\_5,  output logic [15:0] SEXT0\_4 |
| Description | use the highest prior bit to decide whether to extend data by 1 or by 0 |
| Purpose | Used to determine the offset. |

|  |  |
| --- | --- |
| **Modules** | **reg\_file.sv** |
| Inputs | input logic Clk, Reset,  input logic Load,  input logic [2:0] DRMUX, SR1, SR2,  input logic [15:0] Bus\_in |
| Outputs | output logic [15:0] SR1\_out, SR2\_out |
| Description | This module contains registers and MUX which determine the register’s value and output it. |
| Purpose | Act as R0 to R7, the temporary registers to hold temporary values which the LC3 program can use to perform operations such as addition, store, load, write etc. |

|  |  |
| --- | --- |
| **Modules** | **logic\_nzp.sv** |
| Inputs | input logic Clk, Reset,  input logic [15:0] data\_in |
| Outputs | output logic [2:0] nzp |
| Description | This module is the Branch Enable unit for the instruction BR. IR[11:9] are the N, Z, P bits, if the status register match the condition codes, it will set BEN to the result. |
| Purpose | This module determines whether an branch operation should be excuted based on the status register’s number. If it matches with the conditions given in the BR instruction, then the PC is changed. |

|  |  |
| --- | --- |
| **Modules** | **HexDriver.sv** |
| Inputs | input logic [3:0] In0 |
| Outputs | output logic [6:0] Out0 |
| Description | This is a hex driver that transfers a 4-bit signal to represent a hex display on the FPGA. The 4 bits in are needed to have designations for hex values 0 to F. |
| Purpose | It helps to present the output hex-value on the board. |

|  |  |
| --- | --- |
| **Modules** | **tristate.sv** |
| Inputs | input logic Clk,  input logic tristate\_output\_enable,  input logic [N-1:0] Data\_write |
| Outputs | output logic [N-1:0] Data\_read,  (inout wire [N-1:0] Data) |
| Description | This module is a tristate buffer which allow data reads and writes to the SRAM. |
| Purpose | It is used to transmit data to and from MEM2IO and SRAM. |

|  |  |
| --- | --- |
| **Modules** | **test\_memory.sv** |
| Inputs | input Clk,  input Reset,  inout [15:0] I\_O,  input [19:0] A,  input CE, UB, LB, OE, WE |
| Description | This module is the top level of a simulating memory. |
| Purpose | This memory has similar behavior to the SRAM IC on the DE2 board. This file is for simulations only. In simulation, this memory is guaranteed to work at least as well as the actual memory (that is, the actual memory may require more careful treatment than this test memory). At synthesis, this will be synthesized into a blank module. |

|  |  |
| --- | --- |
| **Modules** | **slc3.sv** |
| Inputs | input logic [15:0] S,  input logic Clk, Reset, Run, Continue |
| Outputs | output logic [11:0] LED,  output logic [6:0] HEX0, HEX1, HEX2, HEX3, HEX4, HEX5, HEX6, HEX7,  output logic CE, UB, LB, OE, WE,  output logic [19:0] ADDR,  inout wire [15:0] Data |
| Description | This is the layout of the entire SLC3 processor. It instantiates datapath, MEM2IO, the ISDU, and several other modules and serves as the central glue to hold them all together using the same variable names. |
| Purpose | It is designed to simulate LC3 and glues all the elements of the device together. |

|  |  |
| --- | --- |
| **Modules** | **register.sv** |
| Inputs | input logic Clk, Reset, Load  input logic [15:0] data\_in, |
| Outputs | output logic [15:0] data\_out |
| Description | This module holds 16-bits registers and 12-bits LED register. |
| Purpose | The registers can be used to hold values for the LED and other module need registers. |

|  |  |
| --- | --- |
| **Modules** | **mux.sv** |
| Inputs | input logic SEL,  input logic [k-1:0] A, B |
| Outputs | output logic [k-1:0] Out |
| Description | It includes all muxes, we default that input signals A, B, C, D... are selcted as 0, 1, 2, 3...  It includes 2-to-1 MUX, 4-to-1 MUX, MUX\_bus as mux work as the gate of bus line. |
| Purpose | In this module, for 2 or 4 inputs of the same bit length, the control signal would determine which one is needed and output it through the 2-to-1 MUX or 4-to1 MUX. The gate of the databus is also included in this module. |

|  |  |
| --- | --- |
| **Modules** | **memory\_contents.sv** |
| Description | Store the memory content that may be simulated. |
| Purpose | The memory contents in the test memory. |

|  |  |
| --- | --- |
| **Modules** | **Mem2IO.sv** |
| Inputs | input logic Clk, Reset,  input logic [19:0] ADDR,  input logic CE, UB, LB, OE, WE,  input logic [15:0] Switches,  input logic [15:0] Data\_from\_CPU, Data\_from\_SRAM, |
| Outputs | output logic [15:0] Data\_to\_CPU, Data\_to\_SRAM  output logic [3:0] HEX0, HEX1, HEX2, HEX3 ) |
| Description | This module is made of several muxes, it inputs the address from the MAR and can write and read memory based on the address and the WE and OE bits in the ISDU. |
| Purpose | This allows data transfer between the SLC3 processor datapath and the memory content in SRAM. It also allows data input from the switches as well as data output to the hexdrivers. It allows modification. |

|  |  |
| --- | --- |
| **Modules** | **lab6\_toplevel.sv** |
| Inputs | input logic [15:0] S,  input logic Clk, Reset, Run, Continue |
| Outputs | output logic [11:0] LED,  output logic [6:0] HEX0, HEX1, HEX2, HEX3, HEX4, HEX5, HEX6, HEX7,  output logic CE, UB, LB, OE, WE,  output logic [19:0] ADDR,  inout wire [15:0] Data |
| Description | This is the top level of lab6. It instantiates an instance of slc3 as well as test\_memory. |
| Purpose | It combines SLC-3 processor and the available Test\_memory. |

|  |  |
| --- | --- |
| **Modules** | **ISDU.sv** |
| Inputs | input logic Clk, Reset, Run, Continue,  input logic[3:0] Opcode,  input logic IR\_5,  input logic IR\_11,  input logic BEN, |
| Outputs | output logic LD\_MAR, LD\_MDR, LD\_IR, LD\_BEN, LD\_CC, LD\_REG, LD\_PC, LD\_LED,  output logic GatePC, GateMDR, GateALU, GateMARMUX,  output logic [1:0] PCMUX,  output logic DRMUX, SR1MUX, SR2MUX, ADDR1MUX,  output logic [1:0] ADDR2MUX, ALUK,  output logic Mem\_CE, Mem\_UB, Mem\_LB, Mem\_OE, Mem\_WE |
| Description | This module is the state machine FSM which control the signals on muxes, registers, gates, regfiles to manage the SLC-3 operation process based on instructions. |
| Purpose | It output control signals to contol datapath and other modules though the different states. |

|  |  |
| --- | --- |
| **Modules** | **datapath.sv** |
| Inputs | logic Clk, Reset,  logic LD\_MAR, LD\_MDR, LD\_IR, LD\_BEN, LD\_CC, LD\_REG, LD\_PC, LD\_LED,  logic GatePC, GateMDR, GateALU, GateMARMUX,  logic [1:0] PCMUX, ADDR2MUX, ALUK,  logic DRMUX, SR1MUX, SR2MUX, ADDR1MUX,  logic MIO\_EN,  logic [15:0] MDR\_In, |
| Outputs | logic BEN,  logic [11:0] LED,  logic [15:0] IR,  logic [15:0] MAR,  logic [15:0] MDR,  logic [15:0] PC |
| Description | This module holds all registers, gates, MUXs, MUXs’ select bits and the data bus. |
| Purpose | The module is used for data transfers and instruction decoding. It performs all operations associated with the signals from ISDU and outputs the results. |

|  |  |
| --- | --- |
| **Modules** | **ALU.sv** |
| Inputs | logic [1:0] ALUK  logic [15:0] A,  logic [15:0] B, |
| Outputs | logic [15:0] ALU\_out |
| Description | This is an Arithmetic Logic Unitbuild with some gates and a 4-to-1 MUX. |
| Purpose | It allows basic arithmetic operations and logic operations and it could perform ADD, AND, NOT, or pass one of the input through it depending on the value in ALUK. |

* 1. Block Diagram of slc3.sv
     1. This diagram should represent the placement of all your modules in the **slc3.sv**.

图示, 示意图

描述已自动生成

* 1. Description of the operation of the ISDU (Instruction Sequence Decoder Unit)
     1. Named ISDU.sv, this is the control unit for the SLC-3. Describe in words how the ISDU controls the various components of the SLC-3 based on the current instruction.

It controls the various components of the SLC-3 through various enable bits that are specified in each of the states. As the state diagram of the ISDU shows, the signals would enable or disable the modules based on instructions. Examples of these enable bits are for selecting MUX values, load or store, etc. For example, as the STR instruction is decoded at state 32, the ISDU will next change to stage 7 with signals that first enable RegFile to output baseR, then enable the ALU to ADD the baseR with offset6, then set LD.MAR the to load this value into MAR. After this, it will change to state 23 with signal MIO.EN and LD.MDR to load SR value to MDR. When completed, it will shift to state 16 with signals to store MDR to M[MAR]. When everything completed with complete signal, it will change to state 18 and FETCH stage again.

* 1. State Diagram of ISDU
     1. This should represent all states present in the ISDU and their transitions.

The diagram from Patt & Patel Appendix C can be used as a starting point, but would need to be modified to be representative of the ECE385 implementation of the LC-3. *You will lose points if you just copy the diagram*.

图示

描述已自动生成

1. **Simulations of SLC-3 Instructions**
   1. Simulate the completion of 3 instructions from the following groups: ADD/ADDi/AND/ANDi/NOT; BR/JMP/JSR; LDR/STR. For example, consecutively simulating ADD, BR and then LDR would be an acceptable simulation. You *must* annotate this diagram (for instance, label where instructions begin, where the answer is stored, etc.)
2. **Post-Lab Questions**
   1. Fill out the Design Resources and Statistics table from Post-Lab question one

|  |  |
| --- | --- |
| LUT |  |
| DSP |  |
| Memory (BRAM) |  |
| Flip-Flop |  |
| Frequency |  |
| Static Power |  |
| Dynamic Power |  |
| Total Power |  |

* 1. Answer the following two questions
     1. What is the function of the MEM2IO.sv module?

MEM2IO links the SRAM and the SLC-3 processor. It allows reading from switches, SRAM and writing to the HexDrivers and SRAM

* + 1. What is the difference between the BR and JMP instructions?

JMP changes PC unconditionally, while BR requires that the condition numbers matching the branch nzp bits stored in status register.

* + 1. What is the purpose of the R signal in Patt and Patel? How do we compensate for the lack of the signal in our design? What implications does this have for synchronization?

The R signal is used to confirm that the memory read or write is ready. To compensate for the lack of the signal in our design, we use additional states for the state 33, thus we have 33\_1 and 33\_2 so that the two clock cycles could ensure the memory is ready.

This should have minimal impact on synchronization.

1. **Conclusion**
   1. Discuss functionality of your design. If parts of your design didn’t work, discuss what could be done to fix it
   2. Was there anything ambiguous, incorrect, or unnecessarily difficult in the lab

manual or given materials which can be improved for next semester? You can also specify what we did right so it doesn’t get changed.